**Downloading and installing the pre-trained “wav2vec 2.0” Network:**

downloadFile=matlab.internal.examples.downloadSupportFile("audio","wav2vec2/wav2vec2-base-960.zip");

wav2vecLocation = fullfile(tempdir,"wav2vec");

unzip(downloadFile,wav2vecLocation)

addpath(wav2vecLocation)

**Online verification:**

*hearing\_aid\_features\_demonstration\_vRealTime\_Recording.m*

**Offline verification:**

*hearing\_aid\_features\_demonstration\_Recording.m*

The MATLAB codes were tested on **MATLAB 2023a**.